**5,000 Mile Inspection**

# Mechanic’s Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Bus # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Mileage: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*\*Special Notice\*\* In the event the mechanic is not familiar with the correct clearances, adjustments, specifications, or encounters any other mechanical defect not shown in the following instructions, it will be the mechanic’s responsibility to obtain proper instruction from manufacturer.

INITIAL UPON COMPLETION OF TASK:

Lubrication/Engine: Electrical:

\_\_\_\_\_Clean Engine/Degrease \_\_\_\_\_Check Headlights,Clearance,Turn

\_\_\_\_\_Check All Belts \_\_\_\_\_Check Interior Lights

\_\_\_\_\_Check Oil Level \_\_\_\_\_Check Horn Operation

\_\_\_\_\_Auto Transmission Fluid Level \_\_\_\_\_Check Battery

\_\_\_\_\_Check Rear Axle Oil Level

\_\_\_\_\_Complete Chassis Lube Heating:

\_\_\_\_\_Check Power Steering Fluid Level \_\_\_\_\_Check Heater Cores for Leaks

\_\_\_\_\_Check All Oil Lines & Connections \_\_\_\_\_Check Op. of Blow Motors/Defrosters

\_\_\_\_\_Change/Check All Oil/Air/Fuel Filters \_\_\_\_\_Check Op. of Under Seat Blow Motors

\_\_\_\_\_Check Air Compressor Intake Filter \_\_\_\_\_Check Op. of Booster Pump

\_\_\_\_\_Clean Air Intake Filter Screens

Cooling System: Windshield Wipers:

\_\_\_\_\_Check Coolant Level and Leaks \_\_\_\_\_Check Wiper Operation

\_\_\_\_\_Check Anti-Freeze \_\_\_\_\_Check Washer Operation

\_\_\_\_\_Check All Connections & Fittings \_\_\_\_\_Lube All Wiper Linkage

Suspension & Steering: Interior:

\_\_\_\_\_Check Steering Linkage & Lubricate \_\_\_\_\_Check Driver Seat/Adj./Seat Belt/Lube

\_\_\_\_\_Check Power Steering Hose/Lines \_\_\_\_\_Check All Mirrors

\_\_\_\_\_Visual Wheels/Tires/Check Pressure \_\_\_\_\_Check All Exits, Front & Rear Doors

\_\_\_\_\_Tighten Wheel Nuts/Clock Wheel Roof Hatch/Window Exits/Side Door

\_\_\_\_\_Check Tire Wear for Alignment \_\_\_\_\_Check Fire Extinguisher

\_\_\_\_\_Check Springs for Cracks,Abrasions \_\_\_\_\_Check First Aid Kit

or Other Damage \_\_\_\_\_Check Seats for Vandalism

\_\_\_\_\_Check Body Outriggers \_\_\_\_\_Check All Grab Rails for Tightness

\_\_\_\_\_Check All Windows

Fuel System & Exhaust System: \_\_\_\_\_Check Rear Door –Exit/Alarm/Seal

\_\_\_\_\_Check Fuel Cap Gasket

\_\_\_\_\_Check Fuel Tank for Leaks Wheelchair Lift:

\_\_\_\_\_Check Exhaust System \_\_\_\_\_Check Wheelchair Lift for Proper Op

\_\_\_\_\_Examine All Connections \_\_\_\_\_Check All Fitting Connections for

Proper Operation

Brakes: \_\_\_\_\_Check Roller Track Panel

\_\_\_\_\_Drain Air Tanks V-Groove Rollers for Alignment

\_\_\_\_\_Check & Tighten Air Lines & Connections \_\_\_\_\_Check Platform Panel Hinge for

\_\_\_\_\_Check Brake Lining Alignment, Binding or Wear

\_\_\_\_\_Check Wheelchair Restraints for

Proper Operation